**Pilot**

|  |
| --- |
| **AZ321 Request IFR clearance destination Dublin** |

**ATC**

|  |
| --- |
| **321, Ground, Roger, ready to copy?** |

**Pilot**

|  |
| --- |
| **Ready to copy, 321** |

**ATC**

|  |
| --- |
| **321, cleared to destination Dublin,**  **via SRN5R,**  **initial 4000, expect FL200 10 mins after departure,**  **departure frequency 126.75,**  **Squawk 5041, readback** |

**Pilot**

|  |
| --- |
| **Cleared to destination Dublin.**  **via SRN5R,**  **initial 4000, expect FL200 10 mins after departure,**  **departure frequency 126.75,**  **Squawk 5041, AZ321** |

**ATC**

|  |
| --- |
| **321, Readback is correct, report ready for push and start up** |

**Pilot**

|  |
| --- |
| **Will call ready for push and start up, 321** |

**Pilot**

|  |
| --- |
| **\_\_\_\_\_ Request IFR clearance destination \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** |

**ATC**

|  |
| --- |
| **\_\_\_\_\_ , Ground, Roger, ready to copy?** |

**Pilot**

|  |
| --- |
| **Ready to copy, \_\_\_\_\_** |

**ATC**

|  |
| --- |
| **\_\_\_\_\_ , cleared to destination \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_,**  **via \_\_\_\_\_\_\_\_\_,**  **initial \_\_\_\_\_\_\_\_\_, expect \_\_\_\_\_\_\_\_\_ \_\_\_\_ minutes after departure,**  **departure frequency 126.75,**  **Squawk \_\_\_\_\_\_\_\_\_, readback** |

**Pilot**

|  |
| --- |
| **Cleared to destination Dublin.**  **via \_\_\_\_\_\_\_\_\_,**  **initial \_\_\_\_\_\_\_\_\_, expect \_\_\_\_\_\_\_\_\_ \_\_\_\_ minutes after departure,**  **departure frequency 126.75,**  **Squawk \_\_\_\_\_\_\_\_\_, \_\_\_\_\_** |

**ATC**

|  |
| --- |
| **321\_\_\_\_\_ Readback is correct, report ready for push and start up** |

**Pilot**

|  |
| --- |
| **Will call ready for push and start up, \_\_\_\_\_** |